Abort the process case

The machine should immediately stop doing anything.

Pre-condition:

The machine is sorting discs.

Trigger:

The use wants to immediately stop the machine.

Flow:

The machine stops transporting the discs. And doesn’t put anymore discs on the transporting mechanism. The user is required to remove all discs that are neither in the container unit nor sorted.

Post-condition:

The machine stopped running.

When the machine is sorting discs and the user wants to immediately stop the machine. The machine stops transporting the discs. And doesn’t put anymore discs on the transporting mechanism. The user is required to remove all discs that are neither in the container unit nor sorted. Then the machine has stopped running.