Use case: Stop the machine

Primary Actor: Machine operator

Scope:

Brief: The machine is waiting for the current process to end before it is send into an inactive state .

Post condition: The machine is sent into an inactive state with no process interrupted.

Precondition: The machine is running\*.

Triggers: The STOP button is pressed.

Basic flow:

1. The machine finishes sorting\* the disk currently in the machine
2. The machine enters an inactive state and will not take any more disks form the storage\* unless the START button is pressed.