Motor\_Down  
In the Motor\_Down state, the sorter is moved down.

Motor\_Down\_Stop  
In Motor\_Down\_Stop, the sorter is moved down, after the start/stop button has been pressed.

White\_Wait  
In this state the machine waits until the colour detector has detected a white disc.

White\_Wait\_Stop

The SORT timer for White\_Wait is stopped in this state.